**Pressure gradient – flow through permeability tests**